# Weekly Call (September 6th, 2017)

## Attendees

Dieter Beller  
Gianmarco Bruno  
Italo Busi  
Daniel King  
Yuji Tochio  
Carlo Perocchio  
Young Lee

## Agenda:

### 1) Review of the updated Use Case I-D

- Latest version was uploaded on Thursday 31 Aug on GitHub (Revision 7)  
- Continue to keep CMI out of scope of the Use Case I-D. Considerations on CMI are in the scope of the DT work but not in the scope of this document.  
- Use of external Specification and Standards documents needs to be clarified in the Use Case I-D  
- Remove Virtual Services from Use Case (as CMI discussion currently out of scope)  
  
A VN type 1 request with multi-source/multi-destination at the CMI can be mapped on TE Tunnel configuration at the MPI.  
The MDSC makes a decision about which path to take (e.g., by using Path Computation requests at the MPI).  
The logic used by MDSC to perform this mapping is for further discussion by the DT but out of scope for the current version of the I-D.  
  
**Action: Italo to add text for MAC switching between different ODUFLEX**  
**Action: Italo to check with Sergio regarding the Grey Topology description in section 6.2**   
**Action: Dan to perform editorial review before we submit 03 version**

### 2) AOB

Next DT call is scheduled for next week Wednesday September 13th, 2017 at 3:00pm CEST

## Note Takers

Italo Busi  
Daniel King  
[JavaScript license information](file:///C:\javascript)